SLUSH PUPPY MACHINE

A machine with a brown liquid in it

Description automatically generated

**Operating Manual**



**SLUSH PUPPY OPERATING INSTRUCTIONS**

Thank you for renting our Slush Puppy machine from PartyZone.ie. Please follow the directions below for to make delicious slush puppy’s for your event. If you have any questions or problems, please do not hesitate to contact us at 0852222000 or 0851568667.

**PLEASE READ ALL INSTRUCTIONS BEFORE USE**

****

**PRECAUTIONS**

Carefully read all instructions before operation.

Do NOT immerse any part of this equipment in water.

Keep cord and plug off the ground and away from moisture. Always unplug the equipment before cleaning.

To avoid burns, do NOT touch heated surfaces.

Do NOT place or leave objects in contact with heated surfaces.

Do NOT allow direct contact of this equipment by the public, this machine is NOT to be operated by anyone under the age of 18.

**Electrical Specifications:**

**1000 Watts, 240V 50HZ., 13AMP Plug**

**Make sure to plug in to a dedicated line with the specifications above and that no other appliances are on the same circuit.**

**General Use of the Machine**

**A blender with a cup

Description automatically generated** turn machine on without product in bowl or with only water in bowl. Not to pour product if the helicoidal agitator is not correctly assembled. Pour product into bowl to “max” line (never add a hot product). Do not let product

go below “min” line.  
Refill with refrigerated product when level is halfway bet ween min and max levels. This way there will always be frozen product available for customers.

**A drawing of a hand opening a piece of furniture

Description automatically generated**

The machine is already set with a normal regulation of the slush consistency. To vary the consistency, act as shown in the picture adjusting of 1/4 of turn in a time.

**Slush Function**

**A close-up of a device

Description automatically generated**Plug in machine and turn on main power switch (A), as in picture. To turn the machine off, perform steps in reverse order. To use refrigeration function, turn on **II** power switch(A).

**A close-up of a machine

Description automatically generated**

Turn switch (A) to freeze  
Turn auger switches on for each bowl (C)  
Turn switches (B) to freeze  
To turn the machine off, perform steps in reverse order. To use night function, turn switch (A) on position II

**Daily Cleaning Operation**

A drawing of a water tank

Description automatically generated

To empty bowl: turn power off.  
Drain product. Fill bowl with tepid water. Let stand 15 minutes.

A black arrows pointing to a white cylinder

Description automatically generatedTo re-assemble the clean parts properly, refer to the instructions carefully. The gasket must be set crushing on the bottom of the support. Never apply lubricant to the tank, evaporator pipe and tank seal. PN: The lubricant can only be applied on the tap pin.

A drawing of a machine

Description automatically generated

Assemble the bowl pushing down causing the crushing of the gasket and paying attention that the bowl flits are inside the right guides on the support.

A diagram of a machine

Description automatically generated

For the right spiral assembly, push it down to fix it in the center and then turn in clockwise sense to block it.  
**ATTENTION:** once the spiral is in its right position do not force it and never rotate it by hand. This operation could compromise the working of the motor.

**There is an additional €20 cleaning charge for machines that have not been wiped down or emptied.**

<https://www.youtube.com/watch?v=vJ2sbl__5VY>